दीनदयाल पत्तन प्राधिकरण

 **DEENDAYAL PORT AUTHORITY**



Office of the Superintending Engineer (P),

Administrative Office Building

Post Box No. 50, Gandhidham–Kachchh

Email: seplkpt@gmail.com

[www.deendayalport.gov.in](http://www.deendayalport.gov.in)

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

**No: CN/WK/1611/Ropax/Ghogha/ Date: 21/03/2023**

To,

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_,

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_,

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_,

**Expression of Interest**

**Sub: - Request for EOI for “Annual Maintenance Contract for Link Spans, Pontoons and Terminal facilities at Ghogha.” - Reg.**

Sir,

Deendayal Port Authority intends to carry out the subject work of Project Division of the Civil Engineering Department.

Kindly submit your Expression of Interest along with a budgetary – offer for the items considered in the preparation present market rate under Annexure-I.

The rates quoted must be inclusive of all taxes, duties for performing the scope of work & exclusive of GST. The GST applicable shall be shown separately, which shall not be considered for evaluation purposes.

Your expression of interest along with a budgetary quotation for the above work should reach the following address on or before **24/03/2023 by 15:00 Hrs.**

**Address:-**

Office of the Superintending Engineer (P),

Project Division, Administrative Office Building,

Room No. 221, First floor, Annexe,

P.O. Box No. 50, Gandhidham – Kachchh.

Thanking you,

Yours faithfully,

**Superintending Engineer (P)**

 **Deendayal Port Authority**

**PROJECT DIVISION**

**BUDGETARY OFFER**

**PART - A : FOR WORK AT GHOGHA :-**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Sr.****No.** | **Description** | **Qty.** | **Unit** | **Rate** |
| 1 | Providing and fixing APVC pipes, having thermal stability for hot & cold water supply, including all APVC plain & brass threaded fittings, including fixing the pipe with clamps at 1.00 m spacing. This includes jointing of pipes & fittings with one step APVC solvent cement and testing of joints complete as per direction of Engineer in Charge. |  |  |  |
|  | 1. 15 mm nominal outer dia pipes.
 | 250.00 | 1 R.Mt. |  |
|  | 1. 20 mm nominal outer dia pipes.
 | 200.00 | 1 R.Mt. |  |
|  | 1. 25 mm nominal outer dia pipes.
 | 150.00 | 1 R.Mt. |  |
|  | 1. 40 mm nominal outer dia pipes.
 | 100.00 | 1 R.Mt. |  |
|  | 1. 50 mm nominal outer dia pipes.
 | 50.00 | 1 R.Mt. |  |
| 2 | Operation and maintenance of Linkspan and Pontoon to keep Operational Ropax equipment at all the time that enable to provide uninterrupted services. It broadly includes monitoring / checking / maintain / preventive measures / action and maintenance / repairs activities under different schedule / time line as per Clause No. 5.1 to 5.15 as described in technical specifications in section - 5. The work comprises of all materials, labours, tools, and tackles etc. complete as directed by engineer in charge. | 1.00 | 1 Month |  |

**PART - B : FOR CREDIT PART AT GHOGHA :-**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Sr.****No.** | **Description** | **Qty.** | **Unit** | **Rate** |
| **1** | Taking away dismantled and damaged unserviceable scrap materials which includes MS Channels, plates, bars, angles, barbed wire etc. including loading, unloading & transportation etc. complete as directed by engineer in charge. | 16.90 | 1 M.T. |   |
| **2** | Taking away dismantled doors, windows and clerestory window shutters (steel or wood) including loading, unloading & transportation etc. complete as directed by engineer in charge. | 40.00 | Each |   |
| **3** | Taking away dismantled aluminium/ Gypsum partitions, doors, windows, fixed glazing and false ceiling including loading, unloading & transportation etc. complete as directed by engineer in charge. | 200.00 | 1 M2 |  |